Cardinal 177 RG
Aircraft Performance Specifications

# 177 RG Cardinal

CESSNA AIRCRAFT CORPORATION
| Models 1972 through 1978. Serial numbers 177RG0213 through 177RG1366

General Information |  | 1976 177RG (turbonormalized) Owned by Paul Millner
Engine Make: | Lycoming 200hp
Engine Model: | IO-360-A1B6D
Propeller Type: | McCauley Constant Speed
Power (HP or Lbs Thrust): | 200
Engine TBO: | 2000

S P E E D S (Non-Turbocharged) |  | MPH | KTS | KPH
Maximum Cruising Speed |  | 180 | 156 | 288
Recommended Cruising Speed |  | 171 | 148 | 274
Stalling Speed |  | 57 | 49 | 90

F U E L C A P A C I T Y |  | Lbs | US Gals | Litres
Standard Fuel |  | 402 | 61 | 231
Long Range Version |  | 0 | 0 | 0

W E I G H T S |  |  | US Lbs | Kilos
Gross Weight |  |  | 2800 | 1269
Empty Weight |  |  | 1765 | 800
Max Useful Load |  |  | 1035 | 469
Max Useful w/Full Fuel |  |  | 633 | 287

R A N G E (No Reserve) |  | SM | NM | KM | Hrs
Max Range - Std Cruise |  | 1080 | 888 | 1644 | 6

C E I L I N G S (Non-Turbocharged) |  | Feet | Meters
Max Service Ceiling |  | 17100 | 5211
Max Engine Out Ceiling |  | 0 | 0

C L I M B R A T E S |  | Feet P/Min | Meters P/Min
Max Climb, Sea Level, Gross Weight |  | 925 | 281
Max Climb, Engine Out, Sea Level, Gross Weight |  | 0 | 0

T A K E O F F & L A N D I N G D I S T A N C E S |  | Feet | Meters
TakeOff Ground Roll, Sea Level, Gross Weight |  | 890 | 271
TakeOff Over 50ft/15meter Obstacle, Sea Level, Gross Weight |  | 1585 | 483
Landing Ground Roll, Sea Level, Gross Weight |  | 730 | 222
Landing Over 50ft/15meter Obstacle, Sea Level, Gross Weight |  | 0 | 0

A I R C R A F T D I M E N S I O N S |  | Feet | Meters
Fuselage Length (approx.) |  | 27.3 | 8.32
Fuselage (usually tail section) Height (approx.) |  | 8.7 | 2.65
Total Wingspan (approx.) |  | 35.6 | 10.85