DORNIER Do-Wal CHECKLIST

STATUS: 30.09.02 by W. Beckert
Check the reference tab for plane specs.


____________________________________
Not completed
____________________________________

     Before Starting Engines

1.  Anchor: DOWN (set parking brake)
2.  Battery Switch: ON
3.  Generator: OFF
4.  Pitot: OFF
5.  Navigation Lights : CHECKED
6.  Ailerons: CHECKED
7.  Rudder: CHECKED
8.  Antennas: RETRACTED (use spoilers switch and Navigator Panel)
9.  Trim Wheel: RETURNED TO NEUTRAL
10. Hatches: CLOSED (use SHIFT+E+1 and E+2)
11. Fuel Quantity: CHECKED (max 3640 Liters)
12. Tank Selector: ALL or Main
13. Mixture 1+2: RICH

___________________________________________
   
     Starting Engines 1+2

    --------------------------
1.  Magnets Engine 1: BOTH
2.  Engine 1: START
3.  RPM engine 1: Front (600 RPM)
4.  Oil Pressure 1: CHECKED
5.  Fuel Flow 1: CHECKED
6.  Throttle 1: ADJUSTED
7.  Mixture 1: CHECKED
8.  Magnet 1 R: CHECKED (MAX - 10%)
11. Magnet 1 L: CHECKED (MAX - 10%)  

    --------------------------
1.  Magnets Engine 2: BOTH
2.  Engine 2: START
3.  RPM engine 2: REAR (600 RPM)
4.  Oil Pressure 2: CHECKED
5.  Fuel Flow 2: CHECKED
6.  Throttle 2: ADJUSTED
8.  Mixture 2: CHECKED
9.  Magnet 2 R: CHECKED (MAX - 10%)
10. Magnet 2 L: CHECKED (MAX - 10%) 

___________________________________________

     Before Taxiing/water cruise

1.  Battery Switch: ON
2.  Generator: ON
3.  Pitot: ON
4.  Ailerons: CHECKED
5.  Rudder: CHECKED
6.  Flight Controls: FREE WITH FULL TRAVEL
7.  Tank Selector: ALL ON
8.  Autopilot: OFF 
9.  Radios, Time and Altimeter: CHECKED
10. Altimeters: SET
11. Fuel Quantity: CHECKED
12. MAGS. and GEN: CHECKED
19. Oil Temp. and Press: NORMAL FOR TAKE-OFF
20. Coolant Temp: NORMAL FOR TAKE-OFF (> 60°C)
21. Anchors: UP (release parking brake)
___________________________________________
     Taxiing

1.  Check Turn and Bank Gyro Instruments While taxiing
2.  Do NOT Idle Engines Below 1000 RPM
3.  Check Water Rudder While Taxiing
4.  Direction Compass and Horizon: UNCAGED and SET
5.  ADF: ON, STATION IDENTIFIED AS REQUIRED
6.  Weight and Balance: CHECKED
7.  Trim Wheel: SET FOR TAKE-OFF
8.  Mixture: RICH
9.  Flight Controls: FREE WITH FULL TRAVEL
10. Navigation Lights : AS REQUIRED
___________________________________________
     Before Take-Off

1.  Mixture: RICH
2.  Fuel Valves: ALL TANKS
3.  Altimeter: SET
8.  MAGS. and Generators: CHECKED
9.  Wind Direction: Prefere Headwind
10. Water clear of obstacles: CHECKED
___________________________________________    
     Take-Off

1.  Engines: 1680 RPM
2.  Boat lift on Step: 55 KM/H (about 35 kts)
3.  V1:  80 KM/H
4.  VR:  85 KM/H
5.  V2:  95 KM/H
6.  After Lift off:  Reduce power to 1550 RPM
___________________________________________
     Climb

1.  Autopilot: AS REQUIRED (cheating , he? Better Trim for climb)
2.  Pitot: ON / AS REQUIRED
3.  Altimeter: CHECKED
4.  Vertical Speed: 3.5 m/sec (680 ft p.min) initial climb rate
6.  Oil Pressure 1+2: CHECKED
8.  Coolant Temperature 1+2: CHECKED (below 90 °C)
9.  Fuel Flow 1+2: CHECKED
10. Engines: 1480 RPM MAX
___________________________________________
     Cruise

1.  Autopilot: AS REQUIRED
2.  Airspeed: 180 - 200 KM/H
3.  Altimeter: CHECKED
4.  Gyro Compass: SET and CHECKED
5.  Mixtures: AS REQUIRED
6.  Engines: 1450 RPM max
___________________________________________
     Approach and Landing

1.  Landing Weigth: CHECKED
2.  Autopilot: AS REQUIRED
3.  Oil Pressure 1+2: CHECKED
4.  Pitot: ON
5.  Altimeter: SET
6.  Fuel Selectors: ALL TANKS
7.  Mixtures: RICH
8.  Antenna Wire: RETRACTED (with spoiler key)
9.  Navigation Lights/Landing : AS REQUIRED
___________________________________________
     Landing

1.  Autopilot: OFF (finally, YOU must control the plane)
2.  Altimeter: SET
3.  ADF: AS REQUIRED
4.  Approach:   170 KM/H
5.  Base:       150 KM/H
8.  Final:      130 KM/H
9.  Flare:      130-120 KM/H
10. Touchdown:  120 KM/H (Stall speed < 58 kts)
___________________________________________
     After Landing

1.  Engines: < 1300 RPM
2.  Trim Wheel: Neutral
3.  Pitot Heat: OFF
4.  Mixture: RICH
5.  Taxiing to Anchor Point: Speed below 35 kts
6.  Prepare Anchors
7.  Deploy Teloscopic Antenna Mast: AS REQUIRED
8.  Mixture: Lean
9.  Magnets Engines 1+2: ALL OFF
10. Fuel Cock: CLOSED
___________________________________________
     Secure Aircraft

1.  Anchors: DOWN (set parking brake)
2.  Lights: OFF
3.  Electrical Switches: ALL OFF 
4.  Battery Switch: OFF

